# Inject 06,

## Subject: Records

### Dear Personnel,

Using the Windows Server located within the LAN Network of your router. Provision an A Record for the IP Address of the Containerized LAMP Stack. Meaning, I should be able to do something like <http://yourmom.ayo.deez> and be able to reach your lamp stack that is listening to an IP Address within the 192.168.220.1/24 Network.

As always, provide a detailed description of how you performed the tasked, and provide a screenie showing that the <http://yourmom.ayo.deez> domain is valid and can reach the LAMP Stack

You mustn’t use anything else to provision the A Record beside Windows Server.

Best,

AB